HEATED TWIN TOWER DESICCANT AIR DRYER
Product Introduction
The Heated Twin Tower Desiccant Air Dryer removes moisture before it ever reaches the ring main, delivering a low pressure dew point for applications that demand truly dry air.
Designed, manufactured and tested strictly to ISO9001, GB150, ISO7183 and QS pressure vessel standards, the unit uses international high-purity alumina adsorbent with vacuum negative pressure filling for a long service life. The certified adsorption tank guarantees safety, while the high-strength heater offers high pressure resistance, electric shock resistance and good heating insulation. An intelligent controller displays running parameters in real time, and high-performance pneumatic valves with a low-power solenoid ensure fast, precise response. Multi-layer fiber silencing keeps noise low.
Where it is specified
[bookmark: _GoBack]Typical duties for this series across our installed base.
Air compressor station systems
Oxygen generating station systems
Blast furnace blowers in steel plants
Gas turbines of various capacities
Air conditioning and air supply systems for the chemical fiber textile industry

Product Features
Built to International Standards
Strictly in accordance with ISO9001, GB150 standard, ISO7183 air dryer standard, QS, pressure vessel inspection specifications for design, manufacturing, production and testing to ensure safe and reliable operation of products.
Reasonable Tower Structure
Reasonable tower structure and control procedures to ensure the contact of compressed air and desiccant.
International High-purity Alumina Adsorbent
The adsorbent adopts international high-purity alumina, molecular sieve, vacuum negative pressure filling method, is not easy to be powdered, and has a long service life.
Certified Adsorption Tank
Adopting the adsorption tank with the pressure vessel certificate, the safety performance is guaranteed.
High-strength Heater
The heater has high strength performance, high pressure resistance, electric shock resistance and good heating insulation.
Intelligent Controller
The intelligent controller is used to display the running parameters in real time with high precision, better system stability and easy operation.
High-performance Pneumatic Control Valve
High-performance pneumatic control valve with fast action response, long service life and good stability, equipped with standard low-power solenoid valve, high precision and fast response.
Low Noise
Silencer, multi-layer fiber material, uniquely designed mechanical noise reduction, lower noise.

Working Conditions
	Model
	EQE Series
	EQE-X Series
	EQE-D Series
	EQE-L Series

	Inlet Temp.
	≤ 38 ℃
	≤ 35 ℃

	Inlet Dew Point
	≤10℃
With Refrigerated Air Dryer
	≤38℃
Without Refrigerated Air Dryer
	≤10℃
With Refrigerated Air Dryer
	≤35℃
Without Refrigerated Air Dryer

	Working Pressure
	0.6 ~ 1.0 MPa

	Regeneration Gas Consumption
	≤ 7%

	Inlet Oil Content
	≤ 0.1 ppm

	Pressure Dew Point
	-20 ~ -40 ℃
	-40 ℃
	-70 ℃
	-20 ~ -40 ℃

	Adsorbent
	Activated Alumina
	Activated Alumina
	Activated Alumina + Molecular Sieve
	Activated Alumina

	Control Mode
	Microcomputer Automatic Control


Note: Other requirements can be customized.
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