LASER CUTTING SERIES – INTEGRATED REFRIGERATED AIR DRYER (1.0 ~ 1.6MPA)
Product Introduction
Integrated refrigerated air dryer designed for laser cutting applications, with a stainless steel plate heat exchanger, skid mounted integrated design and three-stage high efficiency filtration, delivering a stable low dew point of 2~10°C.
Product Features
Stainless steel plate heat exchanger — High efficiency, low dew point.
Skid mounted integrated design — Convenient installation and maintenance, use carefree.
Three-stage filtration — Standard cyclone air water separator and three-stage high efficiency filter, effectively filter oil and impurities.
	Item
	Specification

	Inlet air temperature
	≤60°C

	[bookmark: _GoBack]Cooling method
	Air cooling

	Ambient temperature
	2~45°C

	Pressure dew point
	2~10°C

	Working pressure
	0.6~1.6MPa

	Pressure drop
	≤0.05MPa

	Refrigerant
	R410a (Optional R513a)



