MICRO LOSS BLOWER HEAT DESICCANT AIR DRYER
Product Introduction
The micro-loss blower heat series, similar to the zero-loss series, is also divided into two models according to whether the upstream front end is equipped with a chiller: the conventional series with chiller (EQG series) and the reinforced series without chiller (EQG-X series). The front-end refrigerated dryer significantly reduces the water content in the intake air and lowers the load; without it, the water content is many times higher. The two series share the same design principle but differ greatly due to different loads; users should select the corresponding series according to actual conditions.
Standard Working Condition
■  8 ~ 12 hours standard cycle
■  Inlet pressure: 0.6 ~ 1.0 MPa
■  Average regeneration gas consumption: 3 ~ 5%
■  Inlet temperature: ≤ 38 ℃
[bookmark: _GoBack]■  Pressure dew point: ≤ -40 ℃
■  Pressure loss: ≤ 0.021 MPa

Product Features
■  Reliable Adsorption: with a specific surface area of 350 m²/g, this high-efficiency adsorbent developed with upstream suppliers has an excellent adsorption rate to ensure a stable dew point.
■  Durable Performance: vacuum negative-pressure filling ensures tightness and anti-pulverization for longer service life.
■  Intelligent Energy Saving: equipped with a PLC controller for real-time monitoring and data storage, integrating time, load and dew-point control for high energy efficiency.
■  Smart IoT Integration: supports easy remote control, centralized management, intelligent analysis and prediction to optimize operation.
■  Stainless Steel Pneumatic Piping: corrosion-resistant, durable and aesthetically pleasing.
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