MICRO LOSS COMPRESSION HEAT DESICCANT AIR DRYER
Product Introduction
The micro-loss compression heat series is divided into two models according to the exhaust dew point: without heater (EQY, target dew point -20℃) and with heater (EQY-T, target dew point -40℃, customized). The two series are basically the same, except that the with-heater model adds a heater during thermal regeneration so that the adsorbent is desorbed at a higher temperature and regenerated more thoroughly to achieve a lower dew point. In structure, only the heater component is added to the air inlet. Users should select the corresponding series according to actual dew-point requirements.
Standard Working Condition
[bookmark: _GoBack]■  8 hours standard cycle
■  Inlet pressure: 0.6 ~ 1.0 MPa
■  Inlet temperature: ≥ 110 ℃
■  Pressure dew point: -20 ~ -40 ℃ (lower values require customization)
■  Average regeneration gas consumption: 3 ~ 5%
■  Pressure loss: ≤ 0.035 MPa

Product Features
■  Reliable Adsorption: with a specific surface area of 350 m²/g, this high-efficiency adsorbent developed with upstream suppliers has an excellent adsorption rate to ensure a stable dew point.
■  Durable Performance: vacuum negative-pressure filling ensures tightness and anti-pulverization for longer service life.
■  Intelligent Energy Saving: equipped with a PLC controller for real-time monitoring and data storage, integrating time, load and dew-point control for high energy efficiency.
■  Smart IoT Integration: supports easy remote control, centralized management, intelligent analysis and prediction to optimize operation.
■  Stainless Steel Pneumatic Piping: corrosion-resistant, durable and aesthetically pleasing.
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