ZERO LOSS COMPRESSION HEAT DESICCANT AIR DRYER
The zero-loss compression heat series is divided into two models according to the exhaust dew point: without heater (EQY-NLW, target dew point -20℃) and with heater (EQY-NLWT, target dew point -40℃, customized). The two series are basically the same, except that the with-heater model adds a heater during thermal regeneration so that the adsorbent is desorbed at a higher temperature and regenerated more thoroughly to achieve a lower dew point. The with-heater series also includes a patented energy-saving low-dew-point model (EQY-BT) with partial-flow regeneration. Users should select the corresponding series according to actual dew-point requirements.
Standard Working Condition
■  8 hours standard cycle
■  Inlet pressure: 0.6 ~ 1.0 MPa
■  Average regeneration gas consumption: 0%
■  Inlet temperature: ≥ 110 ℃
■  Pressure dew point: -20 ~ -40 ℃ (lower values require customization)
■  Pressure loss: ≤ 0.049 MPa

Product Features
■  Reliable Adsorption: with a specific surface area of 350 m²/g, this high-efficiency adsorbent developed with upstream suppliers has an excellent adsorption rate to ensure a stable dew point.
■  Durable Performance: vacuum negative-pressure filling ensures tightness and anti-pulverization for longer service life.
■  Intelligent Energy Saving: equipped with a PLC controller for real-time monitoring and data storage, integrating time, load and dew-point control for high energy efficiency.
■  Smart IoT Integration: supports easy remote control, centralized management, intelligent analysis and prediction to optimize operation.
■  Stainless Steel Pneumatic Piping: corrosion-resistant, durable and aesthetically pleasing.
■  Patented Design: patented compression-heat shut-down regeneration; low power enables high-temperature regeneration, with lower dew point and higher energy efficiency.
■  Zero Loss Regeneration: no compressed air is consumed throughout the entire cycle, maximizing air-compressor energy savings.




