HIGH EFFICIENCY OIL REMOVER
[bookmark: _GoBack]The EP-HWOS series products use ultra-fine fiber as the main filter material and employ cyclone separation, pre-filter and fine filter, and coagulation fine filter for three-stage purification. When used with an oil-lubricated compressor, it produces gas of similar quality to that of an oil-free lubricating compressor, with high dust removal capacity and some dehumidification and drying ability. It is widely used in pneumatic instruments, automatic control and food, pharmaceutical, chemical, textile, petroleum, spray paint, telecommunications, metallurgy, rubber and other industries.

Working Conditions and Technical Indicators
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	Inlet air pressure
	0.6~1.0MPa
	Initial pressure drop
	≤0.02MPa

	Inlet air temperature
	1.5°C~50°C
	Oil content of outgas
	≤0.01ppm



